**Miami-Dade Police Department**

**Micro Air Vehicle**

**AIR VEHICLE (AV) RECOVERY AND POST FLIGHT CHECKLIST:**

1. Carefully approach AV
2. On AV pod flip down servo switch
3. On AV pod, flip down power switch
4. On AV pod check that all LED’s are out
5. Conduct inspection for visible damage to AV
6. Carry AV to safe area (USE CAUTION DUE TO HOT ENGINE AND MUFFLER SURFACES)
7. Place AV on to starter base
8. Secure latches (4) on starter base
9. If last flight, defuel utilizing DEFUELING CHECKLIST (MANUAL)-APPENDIX O OR DEFUELING CHEKCLIST (E-FUELER)-APPENDIX P and then store using DISASSEMBLY FOR STORAGE CHECKLIST-APPENDIX L
10. If re-launching, prepare AV using RE-LAUNCH CHECKLIST-APPENDIX K