**Miami-Dade Police Department**

**Micro Air Vehicle**

**FUEL MIXING CHECKLIST:**

1. Begin with an empty fuel approved container (1 Gallon or 5 Gallon capacity)
2. Utilizing only 100 LL or Avgas fill container to its safe level (1 Gallon or 5 Gallon)
3. Measure out AMSOIL synthetic oil based on capacity of fuel container
4. 2.5 oz for each gallon of fuel (12.5 oz for 5 gallons) and add to fuel container`
5. Label fuel container with mix date of fuel