**Miami-Dade Police Department**

**Micro Air Vehicle**

**AIR VEHICLE (AV) RE-LAUNCH PROCEDURES CHECKLIST:**

1. Remove AV to refueling area
2. Remove battery cover from top of avionics pod
3. Remove battery and replace with a charged battery
4. Replace battery cover to top of avionics pod
5. Remove excess fuel from AV-If using a manual fuel syringe then proceed to AIR VEHICLE DEFUELING CHECKLIST (MANUAL)-APPENDIX O
6. If utilizing an e-fueler then proceed to AIR VEHICLE FUELING PROCEDURES CHECKLIST (E-FUELER) –APPENDIX N, BEGINNING AT STEP 10
7. After defueling fuel AV for flight-Utilize AIR VEHICLE FUELING CHECKLIST (MANUAL)-APPENDIX M
8. When ready for flight carefully carry AV to launch area
9. Utilize AIR VEHICLE ENGINE START CHECKLIST-APPENDIX H